**2016 TAC Product Review Summary**

|  |  |  |  |
| --- | --- | --- | --- |
| **Manufacturer** | **Product** | **Approval Date**  **(ODH Director)** | **Notes** |
| Ecological Tanks, Inc. | Aqua Aire approved treatment trains  Aqua Safe approved treatment trains Control Panel Model 209 | 5/17/2016 | Approval modification for Aqua Aire and Aqua Safe treatment trains approved for spray irrigation to allow two different timers (209-H and 209-R) for control panel Model 209. |
| Premier Tech Aqua | Ecoflo Coco Filter | 5/17/2016 | Approval of Premier Tech Aqua Coco Filter models for meeting the treatment standards of five-day carbonaceous biochemical oxygen demand and total suspended solids for sizing reduction. |
| Consolidated Treatment Systems | Flow2 Ultraviolet | 8/15/2016  12/5/2016 | Approval of the Flow2 ultraviolet disinfection unit (F2-UV) as a substitute for ultraviolet disinfection in previously approved treatment trains with a concurring request from the manufacturer of the approved treatment train. Product is approved for:   * One-foot soil depth credit (8/15/16) * Two-foot soil depth credit (12/5/16) * NPDES discharge (12/5/16) |
| Anua (formerly Bord na Mona) | Puraflo polishing (tertiary) filter | Manufacturer withdrew application 5/3/2016 | Request for approval of the Puraflo Peat Fiber Biofilter Polishing Filter as a tertiary component or device. |
| Anua (formerly Bord na Mona) | Type A Peat Biofilter  Type B Peat Biofilter | Manufacturer withdrew application 5/3/2016 | Request for modification of previous approvals to increase loading rates for Type A and Type B Peat Biofilter systems. |
| Norweco, Inc. | Singulair 960-500 and  Singular Green TNT 500 | 9/12/2016 | Modification of previous approval to utilize a new tank design. |
| Consolidated Treatment Systems | Multi-Flo and Enviro-Guard treatment trains | 11/2/2016 | Modification of previous approvals to allow use of alternative pumps and control panels for previously approved Consolidated Treatment Systems Inc. treatment trains utilizing Multi-Flo and Enviro-Guard units. |
| Consolidated Treatment Systems | Nayadic MV6 Evolution Tank | 1/19/2017 | Modification of previous approvals of the Consolidated Treatment Systems, Inc. Nayadic systems to include M6-Evolution tank configurations. |
| Consolidated Treatment Systems | Enviro-Guard, Nayadic, Multi-Flo, and Sybr-Aer treatment trains | 1/19/2017 | Modification of previous approvals to allow the use of ODH approved tanks for pump/dose tanks, trash tanks, and UV/re-aeration tanks, |
| Earthbuster | Earthbuster | Denial and notice of opportunity for hearing  1/31/17 | Earthbuster™ 2015 approval request for soil de-compaction equipment remediation product. |